**Top-Coat**

**One layer of Hydro is 15-20 ml**

**(Regular Size Car)**

|  |
| --- |
| ***Preparation*** |
| **Controlled Environment:**- Ensure the application area maintains temperature and humidity control during and for at least 10 hours after application**Washing and Decontaminating:**- Clean your vehicle with an Iron remover to get rid of iron particles.- Use a Mineral remover to remove mineral deposits.- Wash and decontaminate your vehicle using TAR remover- If needed, use a clay bar to eliminate any tough contaminants.**Polishing and Smoothing:**- Compound and polish the vehicle to fix any imperfections and ensure a smooth surface.**Surface Prep:**-Highly recommended to use Titan Bioprep as it will enhance the bonding and remove any residue and silicon deposits.-If you don’t have BioPrep: Wash the car with dish soap solution and wipe down the car first with silicone remover (If polishing compound is silicone based).-Use IPA to wipe down the surface. |

|  |
| --- |
| ***Application*** |
| **Product Application:*** Apply enough drops of Hydro TX145 to your applicator and apply thickly.
* Spread a puddle line and work in a crosshatch pattern slowly.
* The size of the application area can be 50\*50cm panels or follow the bodylines of the car.

**Residue Removal:*** Wipe off immediately with a new quality short pile microfiber until most residue is removed.
* Follow up with a second short pile microfiber to ensure all residue is removed.
* Buff with a new quality long pile microfiber.

**Final Inspection:*** + Once applied and removed, inspect the surface with a long pile microfiber under a bright, diffused light source to ensure no residue remains.

**Layering:*** + Apply the second layer of Hydro TX145 immediately after the first layer.

**Post-Application:*** + Apply Ultra 4.0 after 2 hours.
	+ Do not expose your vehicle to the elements for at least 8 hours.
* -Avoid washing the vehicle for the first 14 days to allow the coating to cure fully.
 |

***NOTES***

 ***Application Volume:***

 ***- Two layers of Hydro back-to-back average approximately 30ml.***

 ***Maintenance Schedule:***

***- Reapply Hydro every 2-3 years for optimal performance.***

***- Change your applicator and microfibers as needed to maintain quality application.***

***- Apply Ultra 4.0 every 3-6 months to enhance protection and gloss.***

***-If you are reskinning using Hydro after 2-3 years, then surface prep is a must before applying.***

***HANDLING***

***Store the coatings in the fridge, Recommended Temperature is 40-48 F.***

***Before Using: Take the coating out of fridge,***

***and let it set for 10-15 minutes and then Shake the bottle for 30 seconds before using.***

***All Coatings are based on elastomer technology***