**One layer of Hyper Glass for the WindShield is 5-10ml only**

|  |
| --- |
| ***Preparation*** |
| **Controlled Environment:**   * Ensure the application area is temperature and humidity controlled during and for at least 10 hours after application.   **Wash and Decontaminate:**   * Use a clay bar to remove hard-bonded contaminants from the glass.   **Glass Polish:**   * Clean and prepare the glass surface with glass polish for further prepare.   **Wipedown:**   * Wash the glass with a dishwashing solution.   **Final Wipedown:**   * Highly recommended to use Titan Bioprep as it will enhance the bonding and remove any residue and silicon deposits. * If you don’t have BioPrep:   Wash the car with dish soap solution and wipe down the car first with silicone remover (If polishing compound is silicone based).   * Use IPA to wipe down the surface. |

|  |
| --- |
| ***Application*** |
| **Apply the Coating:**   * Apply 15-20 drops of Hyperglass to your applicator. * Apply the product thickly. * Reapply product to your applicator if it gets too dry during application. * Apply only one layer of Hyperglass in a circular motion, followed by a crosshatch pattern. * A second layer is not required and may compromise performance.   **Residue Removal:**   * Remove the residue after 15-20 minutes.   **Exposure:**   * Do not expose the glass to the elements for at least 10 hours. * Do not wash the glass for the first 14 days. |

***NOTES***

***HANDLING***

**IR Lamp:**

An IR lamp can be used to speed up the curing process.

**Wiper Blades:**

* If the wiper blades are not new, replace them with a new set
* Coat the wiper blades with Hyperglass.

***Store the coatings in a cold, dry and dark place.***

***Before using, Shake the bottle for 30 seconds***

***Close the bottle after each use***