|  |
| --- |
| ***Product Information*** |
| Ultra V4 is a highly concentrated, water-based hybrid topcoat designed to prevent water spotting and prolong the life of professional-grade coatings. Suitable for all types of ceramic coatings, it is eco-friendly, economical, and effective with just 1 spray per 40x40cm or 1600cm².  **Ultra V4 provides:**   * **Hypergloss** and immediate weather readiness. * A sacrificial, elastic, and flexible layer for self-cleaning. * Protection against ceramic coating degradation. * Performance in all climates and weather systems. * An anti-static polymer for anti-dusting properties.   **Ideal for:**   * Paint systems, wraps, PPF, glass, wheels, and plastic trim. * Standalone coating to add self-cleaning abilities to any surface. |

|  |
| --- |
| ***Application*** |
| **Spray and Work In:**   * Spray directly once or twice onto a new, quality short pile microfiber. * Work the product into the paint surface.   **Buffing:**   * Buff the area with a new, quality long pile microfiber to remove any remaining residue.   **Final Inspection:**   * Perform a final check with your long pile microfiber and a bright, diffused light source to ensure no residue remains on the surface.   **Curing:**   * We advise to use Titan Bioprep to prep the surface * Do not expose your vehicle to the elements for at least 6 hours. |

***HANDLING***

***Store the coatings in a cold, dry and dark place.***

***Before using, Shake the bottle for 30 seconds***

***Close the bottle after each use***

One layer of Ultra is 20-25 ml

(Regular size car)

* Ultra V4 adds Zero Hardness.
* Ultra V4 can be layered immediately.
* Applying Ultra V4 can cause haze or smears if applied on Titan or Zeus coatings that are not fully cured (5 days). This is normal.
* Two layers of Ultra V4 are recommended.
* Never apply Ultra V4 in direct sunlight.
* Ultra V4 can be applied wet or used as a drying aid.
* If applying Ultra 4.0 during maintenance, there is no need for preparation work. Just wash, decontaminate, and apply.

***NOTES***