***OMNIGUARD™ Quick Sealant Application Guide***

**Introduction**

OMNIGUARD™ is a revolutionary quick sealant designed to bridge the gap between quick detailers and traditional sealants. With its advanced formula featuring **HYPERBEAD™ particles**, it offers superior self-cleaning abilities, UV protection, and reduced surface oxidation. Ideal for automotive, marine, and household applications, OMNIGUARD™ is a versatile solution for professionals and enthusiasts alike.

|  |  |
| --- | --- |
| ***Dilution Instructions*** | ***Surface Suitability*** |
| **OMNIGUARD™ is provided in a 50ml concentrate bottle. To prepare the solution:**   * Mix Ratio: Combine 50ml of OMNIGUARD™ concentrate with 950ml of deionized or distilled water. * Container: Use a clean, high-quality spray bottle for mixing and storage. * Storage: Once mixed, the solution is effective for up to 2 years. Ensure the container is sealed tightly when not in use. | **OMNIGUARD™ is safe and effective for use on the following surfaces:**   * Paint finishes * Paint protection film (PPF) * Vinyl wraps * Glass * Wheels * Leather * Marine surfaces * Household surfaces |

**Additional Notes**

* **Durability**: The applied sealant is effective for up to **6 weeks**.
* **Maintenance**: Use OMNIGUARD™ as part of your regular maintenance routine to enhance and extend the protection of your vehicle or surface.
* **Storage Conditions**: Keep the solution in a cool, dry place. Avoid direct sunlight.

|  |
| --- |
| ***Application Instructions*** |
| **Step 1: Prepare the Surface**   * Ensure the surface is clean and free from heavy dirt or debris. * For optimal results, wash and dry the surface before application. * We advise to use Titan Bioprep to prep the surface   **Step 2: Apply OMNIGUARD™**   * **Spray**: Lightly spray OMNIGUARD™ onto a new, high-quality **short-pile microfiber cloth**. * **Work the Product**: Gently work the product into the surface using even, overlapping motions. Avoid letting the product dry before buffing.   **Step 3: Buff the Surface**   * Use a new, high-quality **long-pile microfiber cloth** to buff the surface. * Ensure all remaining residue is removed for a flawless finish.   **Step 4: Final Inspection**   * Inspect the surface using a **bright but diffused light source** to check for any remaining residue. * If residue is found, wash it off with water and buff again if necessary. |

**Key Benefits**

* **Quick Application**: Perfect for pre-delivery wipe downs and maintenance cleaning.
* **Enhanced Protection**: Self-cleaning properties and UV resistance reduce oxidation and keep surfaces looking fresh.
* **Versatility**: Suitable for a wide range of surfaces, including marine and household use.